==============================================================================
                         FUJITSU DL3850+ Printer Driver

                 Copyright(C) 2010-2014 FUJITSU ISOTEC LIMITED
==============================================================================

This printer driver works on the following operating systems:

  Windows(R) 8.1 Enterprise x64 Edition,
  Windows(R) 8.1 Enterprise,
  Windows(R) 8.1 Pro x64 Edition,
  Windows(R) 8.1 Pro,
  Windows(R) 8.1 x64 Edition,
  Windows(R) 8.1
  -> referred to as Windows 8.1
  Windows(R) 8 Enterprise x64 Edition,
  Windows(R) 8 Enterprise,
  Windows(R) 8 Pro x64 Edition,
  Windows(R) 8 Pro,
  Windows(R) 8 x64 Edition,
  Windows(R) 8
  -> referred to as Windows 8

  This printer driver does not support Windows(R) 8.1 RT and Windows(R) 8 RT.


This printer driver is for FUJITSU DL3850+ printers.



Content

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup method using Add Printer Wizard
4. Uninstalling the printer driver
5. Printer driver setup method
6. Others
- About the trademark

Note: This driver is for FUJITSU DL3850+ printers.
      Do not use with other printers.
      When printing using Windows 8.1 and Windows 8, change the printer
      settings back to the factory default.
      Otherwise the printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the Windows 8.1 and Windows 8

- Operating system
  Windows 8.1
  Windows 8



2. Printer driver configuration

  FUJITSU DL3850+ printer driver consists of the following files:

   DL3850.DLL     FUJITSU DL3850+ printer driver resource DLL file
   DL3850.GPD     FUJITSU DL3850+ printer driver GPD file
   NRBMONN.DLL    FUJITSU DL3850+ Language Monitor
   DL3850.INF     Setup information file
   DL3850TH.CAT   Security Catalog file
   README.TXT     This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) Printer Driver Disk (this disk)

- When setting up, log on with an Administrator account.

- If the FUJITSU DL3850+ printer driver has already been set up,
  delete it and set up again.

- This guide includes procedures on installing printer drivers on locally
  connected PC's.
  For installation methods on network connection and shared printers, refer to
  the Windows 8.1 and Windows 8 user's manual or "help".

- During setup, in the User Account Control dialog box, you may be asked, Do
  you want to allow the following program from an unknown publisher to make
  changes to this computer ? Select Yes.

- When using 64-bit Windows 8.1 and 64-bit Windows 8, follow the above
  procedure also.


-----------------------------------------
3.2 Setup method using Add Printer Wizard
-----------------------------------------
Use the Add Printer Wizard to set up the printer driver.
In this section, the setup procedure for Windows 8 is described.
In the following procedure, Fujitsu DL3850+ printer driver is set up.
When using another printer or another printer driver, change it to your current
printer or printer driver name to follow the procedure.

   -NOTE-
   ** The [User Account Control] dialog box may appear during the procedure.
      The dialog box asks for your permission to continue.  Click [Yes].

  1. Press the Windows logo key + X key, shortcut menu is displayed bottom
     left of the screen.

  2. Click [Control Panel], and select [View Devices and Printers].
     Then select [Add a printer] in [Devices and Printers] Folder.

  3. When the [Add a printer] wizard is displayed.
     "Searching for available printers..." is appeared, click the [Next] button.
  4. Then "Find a printer by other options" is appeared, select [Add a local
     or network printer with manual settings], and click the [Next] button.

  5. Specify which port the printer will connect to, and then click the [Next]
     button.
     ** If a port is not available, for example, in a case where a port to
        connect the printer is not present in the list of Use an existing port,
        select a temporary port such as LPT1:(Printer Port) instead.

  6. Select [Have Disk] when the [Install the printer driver] screen is
     displayed."

  7. Insert this disk in the CD or DVD drive (D:) and change the path from
     "A:\" to "D:\DL3850+\Win8".
     ** The CD or DVD drive is set to "D:" in the above example.
        If your CD or DVD drive is set to another driver, change the path to
        the correct drive.
     ** For 64-bit Windows 8.1 and 64-bit Windows 8, the above folder should
        be specified as well.
     ** When installing another printer driver, change the printer driver part
        to your model's printer drive name in the path to specify.
     ** When using the latest printer driver downloaded from our web site, type
        "(a folder name where downloaded driver data is present)\WIN8".
     ** When click the [Browse] button, [Locate File] is displayed.
        Select the location where the driver data is stored, and click [WIN8]
        and [Open] from the displayed file.
        Click [OK] in the screen of [Install From Disk]

  8. Several model names will be displayed in a list box.
     Select [Fujitsu DL3850+], and then click the [Next] button.
     ** If "Which version of the driver do you want to use?" is displayed,
        select [Replace the current printer]."

  9. When the [Type a printer name] window is displayed, enter the printer
     name (to change the printer name, enter the new printer name), and then
     click the [Next] button."

 10. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 11. The wizard will start copying files.

 12. Specify whether to share the printer.
     Select [Do not share this printer], and then click the [Next] button."

 13. Make sure that the message, You've successfully added Fujitsu DL3850+, is
     displayed, and click the Finish button to terminate the wizard.
     ** If multiple printer drivers have been installed, this window will
        display the item, Set as the default printer. Select as needed.
     ** In this window, Print a test page is displayed. If required print a
        test page.
     ** Notes on test page printing
        (1) When a temporary port is selected in Procedure 5., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
            In the printer driver default, Paper Source: Automatically Select
            and Paper Size: Letter are configured.
            Print test pages with Letter-sized cut sheet.
        (4) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 14. Restart Windows. This completes the printer driver setup.

When the printer is connected after the setup in this method, the dialog
Installing device driver software may be displayed and the connected printer
may be displayed under Unspecified part of Devices and Printers.
In that case, restart Windows. 



4. Uninstalling the printer driver

   The following procedure is used to delete the printer driver. 

   -NOTE-
   ** In this section, FUJITSU DL3850+ printer driver is used as an example.
   ** When using another printer driver, change the name to your current
      printer driver name to read the description.
   ** To delete, make sure the printer driver is not in use. If any printing
      is in progress, cancel the printing job.
   ** The User Account Control dialog box may appear during the procedure.
      The dialog box asks for your permission to continue.  Click [Yes].
   ** "Click the [Change Driver Settings] button" will not appear on the menu
      during the following
      procedure if:
        - User Account Control is disabled in the OS.

  1. Press the Windows logo key + X key, shortcut menu is displayed bottom left
     of the screen.
     Then select [Control Panel] and select [View Devices and Printers].

  2. Select [Fujitsu DL3850+] in [Priters and Faxes] area , and click [Remove
     device].

  3. The [Are you sure you want to remove this device ? 'Fujitsu DL3850+']
     dialog box is displayed. Click [Yes].

  4. Select "Fax" or "Microsoft XPS Document Writer" in [Priters and Faxes]
     part, and click [Print server properties].

  5. Click the [Drivers] tag, and click [Change Driver Settings].

  6. Select [Fujitsu DL3850+] in the list of [Installed printer drivers], and
     then click [Remove].

  7. The [Remove Driver And Package] screen is displayed.
     Select [Remove driver and driver package] and click [OK].

  8. The [Deleting this printer driver package will remove it from the system.
     Are you sure you want to delete 'Fujitsu DL3850+' ? ] dialog box is dis-
     played. Click, [Yes].

  9. When [Driver package information collected.] are displayed in [Remove
     Driver Package] dialog box, Click [Delete].

 10. When deletion of the driver is completed, click [OK]. 
     Click [Close] to exit the [Print Server Properties] dialog.

 11. Turn off the power of the printer and restart the computer.

This completes the printer driver removal.
When the following message is displayed in Procedure 9.: This package
contains the following driver(s) that are in use:, restart Windows and
remove the printer driver again.



5. Printer driver setup method

- Document properties such as paper size and others can be set in the "printer
  properties" menu in the application software.

- Depending on the application software used, the paper size settings
  of the application software may be the default rather than that of the
  "page setting" tab.

- How to assign paper size etc to each paper feed is as follows.
  In this section, FUJITSU DL3850+ printer driver is used as an example.
  When using another printer driver, change it to your current printer driver
  name to follow the procedure.
  (1) Select Start, and then select Devices and Printers.
  (2) Right click on Fujitsu DL3850+ displayed under Printers and Faxes and
      select Printer properties.
      Then, specify in the Form To Tray Assignment section under the Device
      Settings tab.
      NOTE:
      - This method is valid only when the Paper Source setting of the printer
        driver is set at the "Automatically Select".
      - Please make sure the actual paper size matches the selected paper size.
        Use the "Manual Paper Feed" the actual paper size differs from the
        selected paper size.

- How to create a user-defined paper size is as follows.
  In this section, Fujitsu DL3850+ printer driver is used as an example.
  When using another printer driver, change it to your current printer driver
  name to follow the procedure.
  (1) Log in with an administrator group account.
  (2) Select Start, and then select Devices and Printers.
  (3) Click Fujitsu DL3850+ displayed under Printers and Faxes and select Print
      server properties on the menu bar.
  (4) Click the Change Form Settings button under the Form tab.
  (5) Check mark Create a new form.
  (6) Type a paper name to create in Form name.
  (7) Select a unit of the paper size to create under Form description
      (measurements) and enter the width and the height of the paper.
  (8) Click Save Form.
  (9) Click the OK button and close Print server properties.
  NOTE:
  - For some versions of Windows 8.1 and Windows 8, the procedure or display
    contents may vary.
    In that case, follow the displayed instructions.
  - Use inch as a unit to specify the length if you can.
  - If a special continuous paper form such as paper length with 10, 11, 13,
    14, 16, or 17 inches in 3 pages as a user-defined size is created or
    configured, an error may occur. This may result in a printing misalignment.
  - For a user-defined size, even after its margins are correctly set, it may
    not be reflected properly. Edit margins in Page Setting in the application.



6. Others

a. The emulation for this driver is in the "ESC/P2" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from other Windows application software under the Windows 8.1 and
   Windows 8 environments may give different results.

d. The contents of "Properties" of the printer driver and "Printing
   Preferences" of the printer may overlap.
   Please make necessary adjustments to avoid any possible malfunction.

e. Paper size from the "Server Properties" can be set to a maximum width of
   15 inches.  Adjust the right and left margins not the exceed an 13.6 inch
   paper width as the data may not be properly printed.

f. When printing with a "Page per Sheet" specification from the "layout" tab
   in the print menu, frame lines may not be printed with some applications.

g. Paper with a length of 3 inches - 14 inches isruled with a width of
   15 inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

h. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

i. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

j. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm.
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

k. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Both the top and bottom margins are set at 25.4mm in this printer driver.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

l. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

m. The DL3850+ printer driver to every connecting port will be set if the
   connecting USB port is changed.  (e.g. FUJITSU DL3850+ (copy 2) etc.)
   Since every setting of the printer driver is the initial value, so
   change the setting according to the using state.

n. Changing the paper feed port or paper size with the page setting or
   document setting in the application.
   The margin size outside the print enabled area can be set even when the
   printer driver specified value is not correctly reflected.
   To prevent this, first set the paper feed port and paper size you intend
   to use with printer properties in the printer folder.
   Then change the paper feed port and paper size in the application, or avoid
   setting the margin size outside the print enabled area.  For information on
   the print enabled area (minimal margin size) per individual paper feed ports
   and paper sizes, refer to the Users Manual.

o. Some specified printer fonts from the application may not be used depending
   on the data format.

p. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

q. When Printer Font is specified and print it, change Language setting
   to PAGE850 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.



- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
