
 << Sorry for English >>

==============================================================================
                         Microsoft Windows Server 2008

                         FUJITSU DL3750+ Printer Driver

                 Copyright(C) 2004,2010 FUJITSU ISOTEC LIMITED
==============================================================================

This printer driver works on the following operating systems:

  Microsoft(R) Windows Server(R) 2008 Standard Edition,
  Microsoft(R) Windows Server(R) 2008 Standard x64 Edition,
  Microsoft(R) Windows Server(R) 2008 Enterprise Edition,
  Microsoft(R) Windows Server(R) 2008 Enterprise x64 Edition
  -> Windows Server 2008

This printer driver is for FUJITSU DL3750+ printers.



Content

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup method using Add Printer Wizard (without using Plug & Play)
  3.3 Using Plug & Play
4. Uninstalling the printer driver
5. Printer driver setup method
6. Others
- About the trademark

Note: This driver is for FUJITSU DL3750+ printers.
      Do not use with other printers.
      When printing using Windows Server 2008, change the printer settings
      back to the factory default.
      Otherwise the printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the Windows Server 2008

- Operating system
  Windows Server 2008



2. Printer driver configuration

  FUJITSU DL3750+ printer driver consists of the following files:

   DL3750.DLL     FUJITSU DL3750+ printer driver resource DLL file
   DL3750.GPD     FUJITSU DL3750+ printer driver GPD file
   NRBMONN.DLL    FUJITSU DL3750+ Language Monitor
   DL3750.INF     Setup information file
   README.TXT     This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) Windows Server 2008 operating system
   2) Printer Driver Disk (this disk)

- When setting up, log on with an Administrator account.

- <Windows needs your permission to continue> may be displayed in the <User
  Account Control> dialog box during the setup process.
  If so, select <Continue>.

- If the FUJITSU DL3750+ printer driver has already been set up,
  delete it and set up again.

- This guide includes procedures on installing printer drivers on locally
  connected PC's.
  For installation methods on network connection and shared printers, refer to
  the Windows Server 2008 user's manual or "help".


---------------------------------------------------------------------
3.2 Setup method using Add Printer Wizard (without using Plug & Play)
---------------------------------------------------------------------
Set up the printer by running the Add Printer Wizard. 
The procedure described here assumes that Windows Server 2008 is already
running.

a. Select "Start" -> "Control Panel" -> "Printers".

b. Select "File" -> "Run as administrator" -> "Add Printer..".

c. Select <Add a local printer> when the <Add Printer> wizard is displayed.

d. Specify which port the printer will connect to, and then click the <Next>
   button.

e. Select <Have Disk> when the <Install the printer driver> screen is
   displayed.

f. Insert this disk in the CD drive (D:) and change the path from "A:\" to
   "D:\Win2008".
   ** In this example, the CD drive is drive D:. 
      If another letter is being used for the CD drive letter, change the drive
      letter accordingly.

g. Several model names will be displayed in a list box.
   Select the model to be used, and then click the <Next> button.
   ** If "Which version of the driver do you want to use?" is displayed,
      select <Replace the current printer>.

h. When the <Type a printer name> window is displayed, enter the printer name
   (to change the printer name, enter the new printer name), make settings for
   the default printer, and then click the <Next> button.

i. "Windows can't verify the publisher of this driver software" will be
   displayed in the <Windows Security> dialog box, but select "-> Install this
   driver software anyway".

j. The wizard will start copying files.

k. Specify whether to share the printer, and then click the <Next> button.
   To not share the printer: Select <Do not share this printer>.
   To share the printer    : Select <Share this printer so that others on your
                             network can find and use it> and enter a <Share
                             name>, <Location> and <Comment>.

l. Make sure that "You've successfully added FUJITSU DL3750+" is displayed,
   and then click the <Finish> button to end the wizard.
   The <Print a test page> button will be displayed, so print a test page if
   necessary.
   ** Make sure that the printer is online when printing test pages.
   ** Notes on printing test pages
      - Test pages are printed according to the current printer driver
        settings.
      - The default settings for the printer driver are "Automatically Select"
        for the paper feed method, and "11 inch Stockform(W:15in)" for the
        paper size, so insert 11 x 15 inch Stockform paper before printing
        the test page.
      - To use a non-default paper size, change the settings before printing
        the test page.

This completes the setup procedure for the printer driver.
If the printer is set up using this method, the <Found New Hardware> window may
be displayed when the computer is restarted.
If this happens, perform the setup procedure again.


---------------------
3.3 Using Plug & Play
---------------------
Require: Be sure to turn off the power to both the computer and the printer.

a. Make sure that the printer is connected to the computer, and then turn on
   the power to the printer.

b. Make sure that the printer is online, and then turn on the power to the
   computer and start Windows Server 2008.

c. If the printer is detected successfully, "Windows needs to install driver
   software for your FUJITSU DL3750+" will be displayed in the <Found New
   Hardware> dialog box. 

d. Select <Locate and install driver software (recommended)>.

e. Select <Don't search online>.

f. When "Insert the disc that with your FUJITSU DL3750+" is displayed,
   insert the printer driver disk in the CD-ROM.
   ** If the setup disk has already been inserted in the drive before this
      window is displayed, the <Next> button will be displayed, so click the
      <Next> button.
   ** To use the latest version of the printer driver downloaded from our
      Website, select "-> I don't have the disc. Show me other options."
      and then go to step g.

g. When "Please select the best match for your hardware from the list below."
   is displayed, select the driver in the "D:\Win2008" folder for the
   <Location> description, and then click the <Next> button.
   Go to step i.
   ** In this example, the CD drive is drive D:. 
      If another letter is being used for the CD drive letter, change the drive
      letter accordingly.

h. When the <Windows couldn't find driver software for your device> window is
   displayed, click <Browse my computer for diver software (advanced)>.

i. When the "Browse for driver software on your computer" window is displayed,
   enter "(name of the folder containing the downloaded driver data) \Win2008"
   in the <Search for driver software in this location:> field, and then click
   the <Next> button.

j. "Windows can't verify the publisher of this driver software" will be
   displayed in the <Windows Security> dialog box, but select "-> Install this
   driver software anyway".

k. The plug-and-play wizard will start copying the files.

l. When the <Found New Hardware - FUJITSU DL3750+> is displayed, make sure
   that the message "The software for this device has been successfully
   installed" is displayed, and then select <Close>.

This completes the setup procedure for the printer driver.



4. Uninstalling the printer driver

<Windows needs your permission to continue> may be displayed in the <User
Account Control> dialog box when the printer driver is deleted.
If so, select <Continue>.
The procedure for deleting the printer driver is as follows.

a. Select "Start" -> "Control Panel" -> Printers".

b. Select "FUJITSU DL3750+" from <Printers>, and then select <File> ->
   <Delete>.

c. Select <Yes> when the <Are you sure you want to delete the printer
   'FUJITSU DL3750+' ?> window is displayed.
   ** If no other printer drivers have been installed, the <The default
      printer has been deleted> window will be displayed.
      Click the <Close> button.
   ** If this printer has been set as the default printer, the <The default
      printer has been deleted.  Change your default printer.> window will be
      displayed.  Click the <Close> button.

d. Select <File> -> <Run as administrator> -> <Server Properties>.

e. Click on the <Drivers> tab, and select "FUJITSU DL3750+" from the list
   of <Installed printer drivers>, and then click the <Remove> button.

f. When the <Remove Driver And Package> window is displayed, select <Remove
   driver and driver package>, and then click the <OK> button.

g. When the <Deleting this printer driver package will remove it from the
   system.  Are you sure you want to delete FUJITSU DL3750+ ?> window is
   displayed, click the <Yes> button.

h. When the <Remove Driver Package> window is displayed, click the <Delete>
   button.

i. When the driver has been deleted, click the <OK> button, and then close the
   < Print Server Properties> dialog box by clicking the <Close>.

j. Turn the printer off, and then restart the computer.

This completes the procedure for deleting the printer driver.



5. Printer driver setup method

- Document properties such as paper size and others can be set in the "printer
  properties" menu in the application software.

- Depending on the application software used, the paper size settings
  of the application software may be the default rather than that of the
  "page setting" tab.

- The following is the method for each paper feeding (to set such as paper
  size assignment):
  [for Windows Server 2008]
      Select "Start" -> "Control Panel" -> "Printers".
      "FUJITSU DL3750+", and click on the right button of the mouse, select
      "properties", specify the "Form to Tray assignment" from the "Device
      Settings" tab.
      NOTE:
      - This method is valid only when the Paper Source setting of the printer
        driver is set at the "Automatically Select".
      - Please make sure the actual paper size matches the selected paper size.
        Use the "Manual Paper Feed" the actual paper size differs from the
        selected paper size.

- Refer read the chapter of software in the user's manual for further details.



6. Others

a. The emulation for this driver is in the "ESC/P2" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from other Windows application software under the Windows Server
   2008 environments may give different results.

d. The contents of "Properties" of the printer driver and "Printing
   Preferences" of the printer may overlap.  Please make necessary adjustments
   to avoid any possible malfunction.

e. Some specified printer fonts from the application may not be used depending
   on the data format.

f. Paper size from the "Server Properties" can be set to a maximum width of
   15 inches.  Adjust the right and left margins not the exceed an 13.6 inch
   paper width as the data may not be properly printed.

   The paper length can be set starting from 1inch (about 25.4 mm).
   However, when specifying any of the paper feed ports below, do not specify
   paper 2.76 inches (about 70.0 mm) or less in length.
   Otherwise, the paper will not be properly fed, leading to a paper jam.
   - manual feed
   - CSF #1
   - CSF #2

g. When printing with a "Page per Sheet" specification from the "layout" tab in
   the print menu, frame lines may not be printed with some applications.

h. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

i. Paper with a length of 3 inches - 14 inches isruled with a width of 15
   inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

j. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

k. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

l. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

m. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

n. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

o. Note for sharing printer into Network environment
    -Printer shared by Network environment may not be able to be used with
     Windows Server 2008 because of Windows Firewall.
     In this case, change the exceptional settings of Windows Firewall with
     following procedure.
     1.Select "Start"->"Control Panel"->"Windows Firewall"->"Allow a program
       through Windows Firewall".
     2.When the dialogo box of "Windows Firewall", select "Exceptions".
     3.Check "File and Printer Sharing", and click "OK".

     **In case that the printer installed into Windows Server 2008 is set
       with Network sharing setting, automatically checked to "File and
       printer share".

p. The DL3750+ printer driver to every connecting port will be set if the
   connecting USB port is changed.  (e.g. FUJITSU DL3750+ (copy 2) etc.)
   Since every setting of the printer driver is the initial value, so
   change the setting according to the using state.

q. When Printer Font is specified and print it, change Language setting
   to WCP1252 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.

r. Regarding the DL3750+ Printer
   Ejecting cut sheet paper to the cut sheet table in front sometimes leads to
   wait for removal of a cut sheet (blinking lamp for ejection in front).
   In such cases, remove the paper from the cut sheet table, load the next
   paper, and then press the online switch.

   **The error message displayed when status of wait for removal of a cut
     sheet (blinking lamp for ejection in front) occurs during printing 
     indicates a time out error, not a paper out error.

s. Changing the paper feed port or paper size with the page setting or
   document setting in the application.
   The margin size outside the print enabled area can be set even when the
   printer driver specified value is not correctly reflected.
   To prevent this, first set the paper feed port and paper size you intend to
   use with printer properties in the printer folder.  Then change the paper
   feed port and paper size in the application, or avoid setting the margin
   size outside the print enabled area.  For information on the print enabled
   area (minimal margin size) per individual paper feed ports and paper sizes,
   refer to the Users Manual.



- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
