===============================================================================

  FUJITSU Serial Dot Matrix Printers
  Driver Software Setup

  FUJITSU DL7600Pro/DL7400Pro Printer Driver


                                     Copyright(C) 2016 FUJITSU ISOTEC LIMITED
===============================================================================

This printer driver works on the following operating systems:

  Windows(R) 10 Enterprise x64 Edition,
  Windows(R) 10 Enterprise,
  Windows(R) 10 Pro x64 Edition,
  Windows(R) 10 Pro,
  Windows(R) 10 Home x64 Edition,
  Windows(R) 10 Home,
  Windows(R) 10 Education x64 Edition,
  Windows(R) 10 Education
  -> referred to as Windows 10

  Microsoft(R) Windows Server(R) 2012 R2 Datacenter,
  Microsoft(R) Windows Server(R) 2012 R2 Standard,
  Microsoft(R) Windows Server(R) 2012 R2 Essentials
  -> referred to as Windows Server 2012 R2

  Windows(R) 8.1 Enterprise x64 Edition,
  Windows(R) 8.1 Enterprise,
  Windows(R) 8.1 Pro x64 Edition,
  Windows(R) 8.1 Pro,
  Windows(R) 8.1 x64 Edition,
  Windows(R) 8.1
  -> referred to as Windows 8.1

  Microsoft(R) Windows Server(R) 2012 Datacenter,
  Microsoft(R) Windows Server(R) 2012 Standard,
  Microsoft(R) Windows Server(R) 2012 Essentials
  -> referred to as Windows Server 2012

  Windows(R) 8 Enterprise x64 Edition,
  Windows(R) 8 Enterprise,
  Windows(R) 8 Pro x64 Edition,
  Windows(R) 8 Pro,
  Windows(R) 8 x64 Edition,
  Windows(R) 8
  -> referred to as Windows 8

  Microsoft(R) Windows Server(R) 2008 R2 Enterprise,
  Microsoft(R) Windows Server(R) 2008 R2 Standard
  -> referred to as Windows Server 2008 R2

  Windows(R) 7 Ultimate x64 Edition,
  Windows(R) 7 Ultimate,
  Windows(R) 7 Enterprise x64 Edition,
  Windows(R) 7 Enterprise,
  Windows(R) 7 Professional x64 Edition,
  Windows(R) 7 Professional,
  Windows(R) 7 Home Premium x64 Edition,
  Windows(R) 7 Home Premium,
  Windows(R) 7 Starter
  -> referred to as Windows 7

  Microsoft(R) Windows Server(R) 2008 Standard x64 Edition,
  Microsoft(R) Windows Server(R) 2008 Standard Edition,
  Microsoft(R) Windows Server(R) 2008 Enterprise x64 Edition,
  Microsoft(R) Windows Server(R) 2008 Enterprise Edition
  -> referred to as Windows Server 2008

  Windows Vista(R) Enterprise x64 Edition,
  Windows Vista(R) Enterprise,
  Windows Vista(R) Ultimate x64 Edition,
  Windows Vista(R) Ultimate,
  Windows Vista(R) Business x64 Edition,
  Windows Vista(R) Business,
  Windows Vista(R) Home Premium x64 Edition,
  Windows Vista(R) Home Premium,
  Windows Vista(R) Home Basic x64 Edition,
  Windows Vista(R) Home Basic
  -> referred to as Windows Vista

Note:
  1. This printer driver does not support...
     - Windows(R) 95
     - Windows(R) 98
     - Windows(R) 98 Second Edition
     - Windows(R) Millennium Edition
     - Windows NT(R) 4.0
     - Windows(R) 2000
     - Windows(R) XP
     - Windows Server(R) 2003
     - Windows Server(R) 2003 R2
     - Windows(R) 10 Mobile
     - Windows(R) 10 IoT Core
     - Microsoft(R) Windows Server(R) 2012 R2 Foundation
     - Microsoft(R) Windows Server(R) 2012 Foundation.
     - Server Core.
     - Windows(R) 8 RT and Windows(R) 8.1 RT.




This printer driver is for DL7600Pro/DL7400Pro printers.


Content

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup method using Add Printer Wizard
    3.2.1 Windows 10
    3.2.2 Windows Server 2012 R2 and Windows Server 2012
    3.2.3 Windows 8.1 and Windows 8
    3.2.4 Windows Server 2008 R2
    3.2.5 Windows 7
    3.2.6 Windows Server 2008
    3.2.7 Windows Vista
4. Uninstalling the printer driver
    4.1 Windows 10
    4.2 Windows Server 2012 R2 and Windows Server 2012
    4.3 Windows 8.1 and Windows 8
    4.4 Windows Server 2008 R2
    4.5 Windows 7
    4.6 Windows Server 2008
    4.7 Windows Vista
5. Printer driver setup method
6. About Barcode Printing
7. Others
- About the trademark

Note: This driver is for DL7600Pro/DL7400Pro printers.
      Do not use with other printers.
      When printing using Windows, change the printer settings back to
      the factory default.
      Otherwise the printer may not function as expected.




1. Printer driver operating environment

 - Hardware:
   PC's with the Windows.

 - Operating system:
   Windows 10
   Windows Server 2012 R2
   Windows 8.1
   Windows Server 2012
   Windows 8
   Windows Server 2008 R2
   Windows 7
   Windows Server 2008
   Windows Vista




2. Printer driver configuration

 FUJITSU DL7600Pro/DL7400Pro printer driver consists of the following files:

 DLGZGPE.DLL    Graphic module
 DLGZUIE.DLL    User interface module
 DLGZCMDE.DLL   Commnad & data create module
 DLGZENRE.DLL   Resource module
 DLGZFRRE.DLL   Resource module
 DLGZDERE.DLL   Resource module
 DLGZITRE.DLL   Resource module
 DLGZEARE.DLL   Resource module
 HGETMON.DLL    DL7600Pro language monitor
 MGETMON.DLL    DL7400Pro language monitor
 DL76PRNE.XPB   DL7600Pro printer infomation file
 DL74PRNE.XPB   DL7400Pro printer infomation file
 DLGZEN.CHM     Help file
 DLGZFR.CHM     Help file
 DLGZDE.CHM     Help file
 DLGZIT.CHM     Help file
 DLGZES.CHM     Help file
 DLGZE.INF      Setup information file
 DLGZE.CAT      Security Catalog file
 DLGZ76PE.INI   Printer infomation file
 DLGZ74PE.INI   Printer infomation file
 DLGZVERE.INI   Printer infomation file
 README.TXT     This file




3. Printer driver setup

 ---------------------
 3.1 Before setting up
 ---------------------
 - Prepare the following for setup:
   1) Printer Driver Disk (this disk)

 - When setting up, log on with an Administrator account.

 - IMPORTANT before setting up:
   Install the printer driver before connecting the printer to your personal
   computer.

 - If the FUJITSU DL7600Pro/DL7400Pro printer driver has already been set up,
   delete it and set up again.

 - In this section, FUJITSU DL7600Pro printer driver is used as an example.

 - This guide includes procedures on installing printer drivers on locally
   connected PC's.
   For installation methods on network connection and shared printers, refer
   to the Windows user's manual or "help".

 - During setup, in the User Account Control dialog box, you may be asked, Do
   you want to allow the following program from an unknown publisher to make
   changes to this computer ? Select <Yes> or <Continue>.

 - When using 64-bit Windows, follow the above procedure also.

 - In the setup methods below, "Start" refers to the Windows logo in the bottom
   left of the desktop.

 - To use the printer in a LAN environment, install the print client software.
   When installing this printer driver before installing client software,
   temporarily select a dummy port (such as LPT1:) for the specified printer
   port in the step of adding a printer, as described below.
   Later, assign the actual port to be used to the printer driver during
   client software installation.
   For details on how to install client software, see the online manual for
   LAN User Software.



 -----------------------------------------
 3.2 Setup method using Add Printer Wizard
 -----------------------------------------
 ++++++++++++++++
 3.2.1 Windows 10
 ++++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows 10 is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

 -NOTE-
 ** The [User Account Control] dialog box may appear during the procedure.
    The dialog box asks for your permission to continue.  Click [Yes].

  1. Press the Windows logo key + X key, shortcut menu is displayed bottom
     left of the screen.

  2. Click [Control Panel], and select [View devices and printers].
     Then select [Add a printer] in [Devices and Printers] Folder.

  3. When the [Add a printer] wizard is displayed.
     "Choose a device or printer to add to this PC" is appeared, click the
     "The printer that I want isn't listed" message.

  4. Then "Find a printer by other options" is appeared, select [Add a local
     printer or network printer with manual settings], and click the [Next]
     button.

  5. Specify which port the printer will connect to, and then click the [Next]
     button.
     ** If a port is not available, for example, in a case where a port to
        connect the printer is not present in the list of Use an existing port,
        select a temporary port such as LPT1:(Printer Port) instead.

  6. Select [Have Disk...] when the [Install the printer driver] screen is
     displayed."

  7. Insert this disk in the CD or DVD drive (D:) and change the path from
     "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_DL7400Pro".
     ** The CD or DVD drive is set to "D:" in the above example.
        If your CD or DVD drive is set to another driver, change the path to
        the correct drive.
     ** For 64-bit Windows 10, the above folder should be specified as well.
     ** When installing another printer driver, change the printer driver part
        to your model's printer drive name in the path to specify.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".
     ** When click the [Browse] button, [Locate File] is displayed.
        Select the location where the driver data is stored, and click
        [DL7600Pro_DL7400Pro] and [Open] from the displayed file.
        Click [OK] in the screen of [Install From Disk]

  8. Several model names will be displayed in a list box.
     Select [FUJITSU DL7600ProE], and then click the [Next] button.
     ** If "Which version of the driver do you want to use?" is displayed,
        select [Replace the current printer]."

  9. When the [Type a printer name] window is displayed, enter the printer
     name (to change the printer name, enter the new printer name), and then
     click the [Next] button."

 10. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 11. The wizard will start copying files.

 12. Specify whether to share the printer.
     Select [Do not share this printer], and then click the [Next] button."

 13. Make sure that the message, You've successfully added FUJITSU DL7600ProE,
     is displayed, and click the Finish button to terminate the wizard.
     ** If multiple printer drivers have been installed, this window will
        display the item, Set as the default printer. Select as needed.
     ** In this window, Print a test page is displayed. If required print a
        test page.
     ** Notes on test page printing:
        (1) When a temporary port is selected in Procedure 5., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 14. Restart Windows. This completes the printer driver setup.

 When the printer is connected after the setup in this method, the dialog
 Installing device driver software may be displayed and the connected printer
 may be displayed under Unspecified part of Devices and Printers.
 In that case, restart Windows. 


 ++++++++++++++++++++++++++++++++++++++++++++++++++++
 3.2.2 Windows Server 2012 R2 and Windows Server 2012
 ++++++++++++++++++++++++++++++++++++++++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows Server 2012 R2 / Windows
 Server 2012 is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

 -NOTE-
 ** The [User Account Control] dialog box may appear during the procedure.
    The dialog box asks for your permission to continue.  Click [Yes].

  1. Press the Windows logo key + X key, shortcut menu is displayed bottom
     left of the screen.

  2. Click [Control Panel], and select [View Devices and Printers].
     Then select [Add a printer] in [Devices and Printers] Folder.

  3. When the [Add a printer] wizard is displayed.
     "Searching for available printers..." is appeared, click the [Next]
     button.

  4. Then "Find a printer by other options" is appeared, select [Add a local
     or network printer with manual settings], and click the [Next] button.

  5. Specify which port the printer will connect to, and then click the [Next]
     button.
     ** If a port is not available, for example, in a case where a port to
        connect the printer is not present in the list of Use an existing port,
        select a temporary port such as LPT1:(Printer Port) instead.

  6. Select [Have Disk] when the [Install the printer driver] screen is
     displayed."

  7. Insert this disk in the CD or DVD drive (D:) and change the path from
     "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_DL7400Pro".
     ** The CD or DVD drive is set to "D:" in the above example.
        If your CD or DVD drive is set to another driver, change the path to
        the correct drive.
     ** When installing another printer driver, change the printer driver part
        to your model's printer drive name in the path to specify.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".
     ** When click the [Browse] button, [Locate File] is displayed.
        Select the location where the driver data is stored, and click
        [DL7600Pro_DL7400Pro] and [Open] from the displayed file.
        Click [OK] in the screen of [Install From Disk]

  8. Several model names will be displayed in a list box.
     Select [FUJITSU DL7600ProE], and then click the [Next] button.
     ** If "Which version of the driver do you want to use?" is displayed,
        select [Replace the current printer]."

  9. When the [Type a printer name] window is displayed, enter the printer
     name (to change the printer name, enter the new printer name), and then
     click the [Next] button."

 10. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 11. The wizard will start copying files.

 12. Specify whether to share the printer.
     Select [Do not share this printer], and then click the [Next] button."

 13. Make sure that the message, You've successfully added FUJITSU DL7600ProE,
     is displayed, and click the Finish button to terminate the wizard.
     ** If multiple printer drivers have been installed, this window will
        display the item, Set as the default printer. Select as needed.
     ** In this window, Print a test page is displayed. If required print a
        test page.
     ** Notes on test page printing:
        (1) When a temporary port is selected in Procedure 5., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 14. Restart Windows. This completes the printer driver setup.

 When the printer is connected after the setup in this method, the dialog
 Installing device driver software may be displayed and the connected printer
 may be displayed under Unspecified part of Devices and Printers.
 In that case, restart Windows. 


 +++++++++++++++++++++++++++++++
 3.2.3 Windows 8.1 and Windows 8
 +++++++++++++++++++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows 8.1 / 8 is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

 -NOTE-
 ** The [User Account Control] dialog box may appear during the procedure.
    The dialog box asks for your permission to continue.  Click [Yes].

  1. Press the Windows logo key + X key, shortcut menu is displayed bottom
     left of the screen.

  2. Click [Control Panel], and select [View Devices and Printers].
     Then select [Add a printer] in [Devices and Printers] Folder.

  3. When the [Add a printer] wizard is displayed.
     "Searching for available printers..." is appeared, click the [Next]
     button.

  4. Then "Find a printer by other options" is appeared, select [Add a local
     or network printer with manual settings], and click the [Next] button.

  5. Specify which port the printer will connect to, and then click the [Next]
     button.
     ** If a port is not available, for example, in a case where a port to
        connect the printer is not present in the list of Use an existing port,
        select a temporary port such as LPT1:(Printer Port) instead.

  6. Select [Have Disk] when the [Install the printer driver] screen is
     displayed."

  7. Insert this disk in the CD or DVD drive (D:) and change the path from
     "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_DL7400Pro".
     ** The CD or DVD drive is set to "D:" in the above example.
        If your CD or DVD drive is set to another driver, change the path to
        the correct drive.
     ** For 64-bit Windows 8.1/8 , the above folder should be specified as
        well.
     ** When installing another printer driver, change the printer driver part
        to your model's printer drive name in the path to specify.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".
     ** When click the [Browse] button, [Locate File] is displayed.
        Select the location where the driver data is stored, and click
        [DL7600Pro_DL7400Pro] and [Open] from the displayed file.
        Click [OK] in the screen of [Install From Disk]

  8. Several model names will be displayed in a list box.
     Select [FUJITSU DL7600ProE], and then click the [Next] button.
     ** If "Which version of the driver do you want to use?" is displayed,
        select [Replace the current printer]."

  9. When the [Type a printer name] window is displayed, enter the printer
     name (to change the printer name, enter the new printer name), and then
     click the [Next] button."

 10. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 11. The wizard will start copying files.

 12. Specify whether to share the printer.
     Select [Do not share this printer], and then click the [Next] button."

 13. Make sure that the message, You've successfully added FUJITSU DL7600ProE,
     is displayed, and click the Finish button to terminate the wizard.
     ** If multiple printer drivers have been installed, this window will
        display the item, Set as the default printer. Select as needed.
     ** In this window, Print a test page is displayed. If required print a
        test page.
     ** Notes on test page printing:
        (1) When a temporary port is selected in Procedure 5., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 14. Restart Windows. This completes the printer driver setup.

 When the printer is connected after the setup in this method, the dialog
 Installing device driver software may be displayed and the connected printer
 may be displayed under Unspecified part of Devices and Printers.
 In that case, restart Windows. 


 ++++++++++++++++++++++++++++
 3.2.4 Windows Server 2008 R2
 ++++++++++++++++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows Server 2008 R2 is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

  1. Log on as an administrator of the computer.

  2. Select Start, and then select Devices and Printers. 

  3. From the Devices and Printers folder, select Add a printer. 

  4. The Add Printer Wizard is displayed. Select Add a local printer. 
     ** In Windows Server 2008 R2, the following window is displayed.
        Select Add a local or network printer as an administrator.
        This window is not displayed when you log in using built-in
        administrator account.

  5. Specify a port to connect the printer to and click the Next button.
     ** If a port is not available, for example, in a case where a port to
        connect the printer is not present in the list of Use an existing port,
        select a temporary port such as LPT1:(Printer Port) instead.

  6. The window of Install the printer driver is displayed. Click Have Disk.

  7. Insert the Setup CD-ROM into CD or DVD drive (D:).
     Then, change the path name from "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_
     DL7400Pro" and click the OK button.
     ** The CD or DVD drive is set to "D:" in the above example.
        If your CD or DVD drive is set to another driver, change the path to
        the correct drive.
     ** When installing another printer driver, change the printer driver part
        to your model's printer drive name in the path to specify.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".

  8. The model names are displayed in the list box.
     Select the printer driver to use and click Next. 
     ** When the window containing the message, Which version of the driver do
        you want to use ?, is displayed, select Replace the current driver.

  9. The dialog Type a printer name is displayed. Type the printer name and
     click Next.
     ** To change the printer name, key-in the changed printer name.

 10. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 11. A file copy starts.

 12. The Printer Sharing Window is displayed. Select according to your computer
     environment and click the Next button.
     ** The Printer Sharing Window may not be available for some computer
        environments.
     ** When the Printer Sharing Window is displayed, select according to your
        computer environment.
        (1) Not sharing : Select Do not share this printer. 
        (2) Sharing     : Select Share this printer so that others on your
                          network can find and use it and enter Share name,
                          Location, and Comment.

 13. Make sure that the message, You've successfully added FUJITSU DL7600ProE,
     is displayed, and click the Finish button to terminate the wizard.
     ** If multiple printer drivers have been installed, this window will
        display the item, Set as the default printer. Select as needed.
     ** In this window, Print a test page is displayed. If required print a
        test page.
     ** Notes on test page printing:
        (1) When a temporary port is selected in Procedure 5., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 14. Restart Windows. This completes the printer driver setup.

 When the printer is connected after the setup in this method, the dialog
 Installing device driver software may be displayed and the connected printer
 may be displayed under Unspecified part of Devices and Printers.
 In that case, restart Windows. 


 +++++++++++++++
 3.2.5 Windows 7
 +++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows 7 is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

  1. Log on as an administrator of the computer.

  2. Select Start, and then select Devices and Printers. 

  3. From the Devices and Printers folder, select Add a printer. 

  4. The Add Printer Wizard is displayed. Select Add a local printer. 

  5. Specify a port to connect the printer to and click the Next button.
     ** If a port is not available, for example, in a case where a port to
        connect the printer is not present in the list of Use an existing port,
        select a temporary port such as LPT1:(Printer Port) instead.

  6. The window of Install the printer driver is displayed. Click Have Disk.

  7. Insert the Setup CD-ROM into CD or DVD drive (D:). Then, change the path
     name from "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_DL7400Pro" and click
     the OK button.
     ** The CD or DVD drive is set to "D:" in the above example.
        If your CD or DVD drive is set to another driver, change the path to
        the correct drive.
     ** For 64-bit Windows 7, the above folder should be specified as well.
     ** When installing another printer driver, change the printer driver part
        to your model's printer drive name in the path to specify.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".

  8. The model names are displayed in the list box.
     Select the printer driver to use and click Next. 
     ** When the window containing the message, Which version of the driver do
        you want to use ?, is displayed, select Replace the current driver.

  9. The dialog Type a printer name is displayed. Type the printer name and
     click Next.
     ** To change the printer name, key-in the changed printer name.

 10. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 11. A file copy starts.

 12. The Printer Sharing Window is displayed. Select according to your computer
     environment and click the Next button.
     ** The Printer Sharing Window may not be available for some computer
        environments.
     ** When the Printer Sharing Window is displayed, select according to your
        computer environment.
        (1) Not sharing : Select Do not share this printer. 
        (2) Sharing     : Select Share this printer so that others on your
                          network can find and use it and enter Share name,
                          Location, and Comment.

 13. Make sure that the message, You've successfully added FUJITSU DL7600ProE,
     is displayed, and click the Finish button to terminate the wizard.
     ** If multiple printer drivers have been installed, this window will
        display the item, Set as the default printer. Select as needed.
     ** In this window, Print a test page is displayed. If required print a
        test page.
     ** Notes on test page printing:
        (1) When a temporary port is selected in Procedure 5., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 14. Restart Windows. This completes the printer driver setup.

 When the printer is connected after the setup in this method, the dialog
 Installing device driver software may be displayed and the connected printer
 may be displayed under Unspecified part of Devices and Printers.
 In that case, restart Windows. 


 +++++++++++++++++++++++++
 3.2.6 Windows Server 2008
 +++++++++++++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows Server 2008 is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

  1. Select "Start" -> "Control Panel" -> "Printers".

  2. Select "File" -> "Run as administrator" -> "Add Printer..".

  3. Select <Add a local printer> when the <Add Printer> wizard is displayed.

  4. Specify which port the printer will connect to, and then click the <Next>
     button.

  5. Select <Have Disk> when the <Install the printer driver> screen is
     displayed.

  6. Insert this disk in the CD or DVD drive (D:) and change the path from
     "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_DL7400Pro".
     ** In this example, the CD or DVD drive is drive D:. 
        If another letter is being used for the CD or DVD drive letter, change
        the drive letter accordingly.
     ** For 64-bit Windows Server 2008, the above folder should be specified
        as well.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".

  7. Several model names will be displayed in a list box.
     Select the model to be used, and then click the <Next> button.
     ** If "Which version of the driver do you want to use?" is displayed,
        select <Replace the current printer>.

  8. When the <Type a printer name> window is displayed, enter the printer name
     (to change the printer name, enter the new printer name), make settings
     for the default printer, and then click the <Next> button.

  9. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 10. The wizard will start copying files.

 11. Specify whether to share the printer, and then click the <Next> button.
     To not share the printer: Select <Do not share this printer>.
     To share the printer    : Select <Share this printer so that others on
                               your network can find and use it> and enter a
                               <Share name>, <Location> and <Comment>.

 12. Make sure that "You've successfully added FUJITSU DL7600ProE" is
     displayed, and then click the <Finish> button to end the wizard.
     The <Print a test page> button will be displayed, so print a test
     page if necessary.
     ** Make sure that the printer is online when printing test pages.
     ** Notes on printing test pages:
        (1) When a temporary port is selected in Procedure 4., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 13. Restart Windows. This completes the printer driver setup.

 This completes the setup procedure for the printer driver.
 If the printer is set up using this method, the <Found New Hardware> window
 may be displayed when the computer is restarted.
 If this happens, perform the setup procedure again.


 +++++++++++++++++++
 3.2.7 Windows Vista
 +++++++++++++++++++
 Use the Add Printer Wizard to set up the printer driver.
 In this section, the setup procedure for Windows Vista is described.
 In the following procedure, FUJITSU DL7600Pro printer driver is set up.
 When using another printer or another printer driver, change it to your
 current printer or printer driver name to follow the procedure.

  1. Select "Start" -> "Control Panel" -> "Hardware and Sound" -> "Printers".

  2. Select <Add a printer> from the printer folder.

  3. Select <Add a local printer> when the <Add Printer> wizard is displayed.

  4. Specify which port the printer will connect to, and then click the <Next>
     button.

  5. Select <Have Disk> when the <Install the printer driver> screen is
     displayed.

  6. Insert this disk in the CD or DVD drive (D:) and change the path from
     "A:\" to "D:\SOFTWARE\DRIVERS\DL7600Pro_DL7400Pro".
     ** In this example, the CD or DVD drive is drive D:. 
        If another letter is being used for the CD or DVD drive letter, change
        the drive letter accordingly.
     ** For 64-bit Windows Vista, the above folder should be specified as well.
     ** When using the latest printer driver downloaded from our web site,
        type "(a folder name where downloaded driver data is present)\SOFTWARE
        \DRIVERS\DL7600Pro_DL7400Pro".

  7. Several model names will be displayed in a list box.
     Select the model to be used, and then click the <Next> button.
     ** If "Which version of the driver do you want to use?" is displayed,
        select <Replace the current printer>.

  8. When the <Type a printer name> window is displayed, enter the printer name
     (to change the printer name, enter the new printer name), make settings
     for the default printer, and then click the <Next> button.

  9. "Would you like to install this device software" will be displayed in the
     [Windows Security] dialog box, click the [Install] button.

 10. The wizard will start copying files.

 11. Specify whether to share the printer, and then click the <Next> button.
     To not share the printer: Select <Do not share this printer>.
     To share the printer    : Select <Share this printer so that others on
                               your network can find and use it> and enter a
                               <Share name>, <Location> and <Comment>.
     ** This window will only be displayed if <User Account Control (UAC)> is
        disabled.

 12. Make sure that "You've successfully added FUJITSU DL7600ProE" is
     displayed, and then click the <Finish> button to end the wizard.
     The <Print a test page> button will be displayed, so print a test
     page if necessary.
     ** Notes on printing test pages:
        (1) When a temporary port is selected in Procedure 4., do not print any
            test page.
        (2) Make sure that the printer is online when printing test pages.
        (3) Test pages are printed according to the printer driver settings at
            that point.
        (4) In the printer driver default, Paper Source: Automatically Select
            and Paper Size: 11 inch Stockform(W:15in) are configured.
            Print test pages with 11 inch Stockform.
            When DL7400Pro printer driver default, Paper Source: Automatically
            Select and Paper Size: A4 are configured.
            Print test pages with A4-sized cut sheet.
        (5) To use a non-default feed method or paper size, change the setting
            first, and then print test pages.

 13. Restart Windows. This completes the printer driver setup.

 This completes the setup procedure for the printer driver.
 If the printer is set up using this method, the <Found New Hardware> window
 may be displayed when the computer is restarted.
 If this happens, perform the setup procedure again.




4. Uninstalling the printer driver

 The following procedure is used to delete the printer driver. 

 -NOTE-
 ** In this section, FUJITSU DL7600Pro printer driver is used as an example.
 ** When using another printer driver, change the name to your current
    printer driver name to read the description.
 ** To delete, make sure the printer driver is not in use. If any printing
    is in progress, cancel the printing job.
 ** The User Account Control dialog box may appear during the procedure.
    The dialog box asks for your permission to continue.  Click <Yes> or
    <Continue>.


 --------------
 4.1 Windows 10
 --------------
  1. Press the Windows logo key + X key, shortcut menu is displayed bottom left
     of the screen.
     Then select [Control Panel] and select [View devices and printers].

  2. Select [FUJITSU DL7600ProE] in [Printers] area , and click [Remove
     device].

  3. The [Are you sure you want to remove this device ? 'FUJITSU DL7600ProE']
     dialog box is displayed. Click [Yes].

  4. Select "Fax" or "Microsoft XPS Document Writer" in [Printers] part, and
     click [Print server properties].

  5. Click the [Drivers] tag, and click [Change Driver Settings].
     ** "Click the [Change Driver Settings] button" will not appear on the menu
        during the following
        procedure if:
        (1) User Account Control is disabled in the OS.

  6. Select [FUJITSU DL7600ProE] in the list of [Installed printer drivers],
     and then click [Remove].

  7. The [Remove Driver And Package] screen is displayed.
     Select [Remove driver and driver package] and click [OK].

  8. The [Deleting this printer driver package will remove it from the system.
     Are you sure you want to delete 'FUJITSU DL7600ProE' ? ] dialog box is
     displayed. Click, [Yes].

  9. When [Driver package information collected.] are displayed in [Remove
     Driver Package] dialog box, Click [Delete].

 10. When deletion of the driver is completed, click [OK]. 
     Click [Close] to exit the [Print Server Properties] dialog.

 11. Turn off the power of the printer and restart the computer.

 This completes the printer driver removal.
 When the following message is displayed in Procedure 9.: This package
 contains the following driver(s) that are in use:, restart Windows and
 remove the printer driver again.


 --------------------------------------------------
 4.2 Windows Server 2012 R2 and Windows Server 2012
 --------------------------------------------------
  1. Press the Windows logo key + X key, shortcut menu is displayed bottom left
     of the screen.
     Then select [Control Panel] and select [View Devices and Printers].

  2. Select [FUJITSU DL7600ProE] in [Printers and Faxes] area , and click
     [Remove device].

  3. The [Are you sure you want to remove this device ? 'FUJITSU DL7600ProE']
     dialog box is displayed. Click [Yes].

  4. Select "Fax" or "Microsoft XPS Document Writer" in [Printers and Faxes]
     part, and click [Print server properties].

  5. Click the [Drivers] tag, and click [Change Driver Settings].
     ** "Click the [Change Driver Settings] button" will not appear on the menu
        during the following
        procedure if:
        (1) User Account Control is disabled in the OS.
        (2) You are in a Windows Server 2012 environment, and you have logged
            in with a built-in account (Administrator).

  6. Select [FUJITSU DL7600ProE] in the list of [Installed printer drivers],
     and then click [Remove].

  7. The [Remove Driver And Package] screen is displayed.
     Select [Remove driver and driver package] and click [OK].

  8. The [Deleting this printer driver package will remove it from the system.
     Are you sure you want to delete 'FUJITSU DL7600ProE' ? ] dialog box is
     displayed. Click, [Yes].

  9. When [Driver package information collected.] are displayed in [Remove
     Driver Package] dialog box, Click [Delete].

 10. When deletion of the driver is completed, click [OK]. 
     Click [Close] to exit the [Print Server Properties] dialog.

 11. Turn off the power of the printer and restart the computer.

 This completes the printer driver removal.
 When the following message is displayed in Procedure 9.: This package
 contains the following driver(s) that are in use:, restart Windows and remove
 the printer driver again.


 ---------------------
 4.3 Windows 8.1 and 8
 ---------------------
  1. Press the Windows logo key + X key, shortcut menu is displayed bottom left
     of the screen.
     Then select [Control Panel] and select [View Devices and Printers].

  2. Select [FUJITSU DL7600ProE] in [Printers and Faxes] area , and click
     [Remove device].

  3. The [Are you sure you want to remove this device ? 'FUJITSU DL7600ProE']
     dialog box is displayed. Click [Yes].

  4. Select "Fax" or "Microsoft XPS Document Writer" in [Printers and Faxes]
     part, and click [Print server properties].

  5. Click the [Drivers] tag, and click [Change Driver Settings].
     ** "Click the [Change Driver Settings] button" will not appear on the menu
        during the following
        procedure if:
        (1) User Account Control is disabled in the OS.

  6. Select [FUJITSU DL7600ProE] in the list of [Installed printer drivers],
     and then click [Remove].

  7. The [Remove Driver And Package] screen is displayed.
     Select [Remove driver and driver package] and click [OK].

  8. The [Deleting this printer driver package will remove it from the system.
     Are you sure you want to delete 'FUJITSU DL7600ProE' ? ] dialog box is
     displayed. Click, [Yes].

  9. When [Driver package information collected.] are displayed in [Remove
     Driver Package] dialog box, Click [Delete].

 10. When deletion of the driver is completed, click [OK]. 
     Click [Close] to exit the [Print Server Properties] dialog.

 11. Turn off the power of the printer and restart the computer.

 This completes the printer driver removal.
 When the following message is displayed in Procedure 9.: This package
 contains the following driver(s) that are in use:, restart Windows and
 remove the printer driver again.


 --------------------------
 4.4 Windows Server 2008 R2
 --------------------------
  1. Select Start, and then select Devices and Printers.

  2. Select FUJITSU DL7600ProE under Printers and Faxes. Then, select Remove
     device.

  3. The dialog Remove device is displayed. The message, Are you sure you want
     to remove this device? FUJITSU DL7600ProE, is displayed. Select Yes.

  4. Select the installed printer under Printers and Faxes such as Fax or
     Microsoft XPS Document Writer. Then, select Print server properties.

  5. Click the Drivers tab and click the Change Driver Settings button.
     ** For some log-on accounts, such as a built-in administrator account,
        this button may not be displayed.

  6. From the Installed printer drivers list, select FUJITSU DL7600ProE and
     click the Remove button.

  7. The Remove Driver and Package dialog is displayed.
     Select Remove driver and driver package and click the OK button.

  8. The window containing the message, Deleting this printer driver package
     will remove it from the system. Are you sure you want to delete FUJITSU
     DL7600ProE ?, is displayed. Click Yes.

  9. In the Remove Driver and Package dialog, the following message is
     displayed: Driver package information collected. Click the Delete button.

 10. When the message, Driver package deleted. is displayed, click the OK
     button. 
     Then, click the Close button to terminate the Print server properties
     dialog box.

 11. Turn off the power of the printer and restart the computer.

 This completes the printer driver removal.
 When the following message is displayed in Procedure 10.: This package
 contains the following driver(s) that are in use:, restart Windows and
 remove the printer driver again.


 -------------
 4.5 Windows 7
 -------------
  1. Select Start, and then select Devices and Printers.

  2. Select FUJITSU DL7600ProE under Printers and Faxes. Then, select Remove
     device.

  3. The dialog Remove device is displayed. The message, Are you sure you want
     to remove this device? FUJITSU DL7600ProE, is displayed. Select Yes.

  4. Select the installed printer under Printers and Faxes such as Fax or
     Microsoft XPS Document Writer. Then, select Print server properties.

  5. Click the Drivers tab and click the Change Driver Settings button.
     ** For some log-on accounts, such as a built-in administrator account,
        this button may not be displayed.

  6. From the Installed printer drivers list, select FUJITSU DL7600ProE and
     click the Remove button.

  7. The Remove Driver and Package dialog is displayed.
     Select Remove driver and driver package and click the OK button.

  8. The window containing the message, Deleting this printer driver package
     will remove it from the system. Are you sure you want to delete FUJITSU
     DL7600ProE ?, is displayed. Click Yes.

  9. In the Remove Driver and Package dialog, the following message is
     displayed: Driver package information collected. Click the Delete button.

 10. When the message, Driver package deleted. is displayed, click the OK
     button. 
     Then, click the Close button to terminate the Print server properties
     dialog box.

 11. Turn off the power of the printer and restart the computer.

 This completes the printer driver removal.
 When the following message is displayed in Procedure 10.: This package
 contains the following driver(s) that are in use:, restart Windows and
 remove the printer driver again.


 -----------------------
 4.6 Windows Server 2008
 -----------------------
  1. Select "Start" -> "Control Panel" -> Printers".

  2. Select "FUJITSU DL7600ProE" from <Printers>, and then select <File> ->
     <Delete>.

  3. Select <Yes> when the <Are you sure you want to delete the printer
     'FUJITSU DL7600ProE' ?> window is displayed.
     ** If no other printer drivers have been installed, the <The default
        printer has been deleted> window will be displayed.
        Click the <Close> button.
     ** If this printer has been set as the default printer, the <The default
        printer has been deleted.  Change your default printer.> window will
        be displayed.  Click the <Close> button.

  4. Select <File> -> <Run as administrator> -> <Server Properties>.

  5. Click on the <Drivers> tab, and select "FUJITSU DL7600ProE" from the list
     of <Installed printer drivers>, and then click the <Remove> button.

  6. When the <Remove Driver And Package> window is displayed, select <Remove
     driver and driver package>, and then click the <OK> button.

  7. When the <Deleting this printer driver package will remove it from the
     system.  Are you sure you want to delete FUJITSU DL7600ProE ?> window is
     displayed, click the <Yes> button.

  8. When the <Remove Driver Package> window is displayed, click the <Delete>
     button.

  9. When the driver has been deleted, click the <OK> button, and then close
     the < Print Server Properties> dialog box by clicking the <Close>.

 10. Turn the printer off, and then restart the computer.

 This completes the printer driver removal.


 -----------------
 4.7 Windows Vista
 -----------------
  1. Select "Start" -> "Control Panel" -> "Hardware and Sound" -> "Printers".

  2. Select "FUJITSU DL7600ProE" from <Printers>, and then select <Organize> ->
     <Delete>.

  3. Select <Yes> when the <Are you sure you want to delete the printer
     'FUJITSU DL7600ProE' ?> window is displayed.
     ** If no other printer drivers have been installed, the <The default
        printer has been deleted> window will be displayed.
        Click the <Close> button.
     ** If this printer has been set as the default printer, the <The default
        printer has been deleted.  Change your default printer.> window will
        be displayed.  Click the <Close> button.

  4. Select <Organize> -> <Layout> -> <Menu Bar>.

  5. Select <File> -> <Run as administrator> -> <Server Properties>.

  6. Click on the <Drivers> tab, and select "FUJITSU DL7600ProE" from the list
     of <Installed printer drivers>, and then click the <Remove> button.

  7. When the <Remove Driver And Package> window is displayed, select <Remove
     driver and driver package>, and then click the <OK> button.

  8. When the <Deleting this printer driver package will remove it from the
     system.  Are you sure you want to delete FUJITSU DL7600ProE ?> window is
     displayed, click the <Yes> button.

  9. When the <Remove Driver Package> window is displayed, click the <Delete>
     button.

 10. When the driver has been deleted, click the <OK> button, and then close
     the < Print Server Properties> dialog box by clicking the <Close>.

 11. Turn the printer off, and then restart the computer.

 This completes the printer driver removal.




5. Printer driver setup method

 - Document properties such as paper size and others can be set in the "printer
   properties" menu in the application software.

 - Depending on the application software used, the paper size settings
   of the application software may be the default rather than that of the
   "page setting" tab.

 - How to assign paper size etc to each paper feed is as follows.
   In this section, FUJITSU DL7600ProE printer driver is used as an example.
   When using another printer driver, change it to your current printer driver
   name to follow the procedure.
   -NOTE-
   ** This method is valid only when the Paper Source setting of the printer
      driver is set at the "Automatically Select".
   ** Please make sure the actual paper size matches the selected paper size.
      Use the "Manual Paper Feed" the actual paper size differs from the
      selected paper size.

    [Windows 10]
      (1) Press the Windows logo key + X key, shortcut menu is displayed
          bottom left of the screen.
      (2) Click [Control Panel], and select [View devices and printers].
          Then select [Add a printer] in [Devices and Printers] Folder.
      (3) Right click on Fujitsu DL7600ProE displayed under Printers and
          select Printer properties.
          Then, specify in the Form To Tray Assignment section under the
          Device Settings tab.

    [Windows Server 2012 R2/Windows Server 2012]
    [Windows 8.1/Windows 8]
      (1) Press the Windows logo key + X key, shortcut menu is displayed
          bottom left of the screen.
      (2) Click [Control Panel], and select [View devices and printers].
          Then select [Add a printer] in [Devices and Printers] Folder.
      (3) Right click on Fujitsu DL7600ProE displayed under Printers and Faxes
          and select Printer properties.
          Then, specify in the Form To Tray Assignment section under the Device
          Settings tab.

    [Windows Server 2008 R2]
    [Windows 7]
      (1) Select Start, and then select Devices and Printers.
      (2) Right click on Fujitsu DL7600ProE displayed under Printers and Faxes
          and select Printer properties.
          Then, specify in the Form To Tray Assignment section under the Device
          Settings tab.

    [Windows Server 2008]
    [Windows Vista]
      (1) Select "Start" -> "Control Panel" -> "Printers".
      (2) "FUJITSU DL7600ProE", and click on the right button of the mouse,
          select "properties", specify the "Form to Tray assignment" from the
          "Device Settings" tab.

 - How to create a user-defined paper size is as follows.
   In this section, FUJITSU DL7600ProE printer driver is used as an example.
   When using another printer driver, change it to your current printer driver
   name to follow the procedure.
   -NOTE-
   ** For some versions of Windows, the procedure or display contents may
      vary. In that case, follow the displayed instructions.
   ** Use inch as a unit to specify the length if you can.
   ** If a special continuous paper form such as paper length with 10, 11,
      13, 14, 16, or 17 inches in 3 pages as a user-defined size is created
      or configured, an error may occur.
      This may result in a printing misalignment.
   ** For a user-defined size, even after its margins are correctly set,
      it may not be reflected properly. Edit margins in Page Setting in the
      application.
 
   [Windows 8.1 and later]
    (1) Log in with an administrator group account.
    (2) Press the Windows logo key + X key, shortcut menu is displayed bottom
        left of the screen.
    (3) Click [Control Panel], and select [View devices and printers].
        Then select [Add a printer] in [Devices and Printers] Folder.
    (3) Click FUJITSU DL7600ProE displayed under Printers and select Print
        server properties on the menu bar.
    (4) Click the Change Form Settings button under the Forms tab.
    (5) Check mark Create a new form.
    (6) Type a paper name to create in Form name.
    (7) Select a unit of the paper size to create under Form description
        (measurements) and enter the width and the height of the paper.
    (8) Click Save Form.
    (9) Click the OK button and close Print server properties.

   [Windows 7/Windows Server 2008 R2]
    (1) Log in with an administrator group account.
    (2) Select Start, and then select "Devices and Printers".
    (3) Click FUJITSU DL7600ProE displayed under Printers and Faxes and select
        Print server properties on the menu bar.
    (4) Click the Change Form Settings button under the Form tab.
    (5) Check mark Create a new form.
    (6) Type a paper name to create in Form name.
    (7) Select a unit of the paper size to create under Form description
        (measurements) and enter the width and the height of the paper.
    (8) Click Save Form.
    (9) Click the OK button and close Print server properties.

   [Windows Server 2008/Windows Vista]
    (1) Log in with an administrator group account.
    (2) Select Start, and then select "Printers".
    (3) Select <File> -> <Run as administrator> -> <Server Properties>.
    (4) Check mark Create a new form.
    (5) Type a paper name to create in Form name.
    (6) Select a unit of the paper size to create under Form description
        (measurements) and enter the width and the height of the paper.
    (7) Click Save Form.
    (8) Click the OK button and close Print server properties.




6. About Barcode Printing

  1. The barcode fonts of this printer are defined as printer fonts.
     Although some applications do not display such printer fonts on the font
     list, you can print barcodes by specifying the font to be replaced with
     a barcode font in [Replacement Font].

  2. With some applications, the font specified as barcode may be replaced
     due to font replacement within the application.

  3. Any barcode that is even partially outside the print area of the
     specified paper will not be printed.  The barcode may be outside the
     area because of a setting (such a Width or a Rotation),
     its position, or the number of characters in it.

  4. Notes on barcode data (number of characters)
     - If the number of characters in the specified barcode is less than
       the specified lower limit or greater than the specified upper limit,
       the barcode is not printed.

  5. Do not apply character attributes (such as bold, italic, and outline)
     to the fonts specified as barcode fonts.
     If vertical text or text wrapping is specified for a barcode to be
     printed, the barcode will not be printed normally.

  6. On the application screen, the printing image of barcode is not
     displayed.
     - Adjust the position to make sure that barcode or two-dimensional code
       and surrounding characters are not overlapped each other.
     - The printer cannot print multiple barcodes (two-dimensional codes)
       of the same type on the same line.

  7. Some applications may not notify the printer driver of the space
     character in two-byte or one-byte at the end of the character string
     properly.
     When the character string containing the space character in two-byte or
     one-byte at the end is specified as barcode in such application, 
     barcode may not be printed as expected.

  8. Note on Code 39 barcodes
     - Specify the alphabets (A to Z) in capital letters.
     - The start, stop codes (*) are added automatically in the printer
       side.
     - When the character string contains '*', the character string is
       printed as far as '*' and the rest of the character string is
       printed as normal characters.

  9. Note on Code128 barcodes
     - Add the start code ({A,{B,{C) at the beginning of the character string.
       Without the start code, Code 128 barcode cannot be printed.
     - With the start code C, specifying code or function is not allowed
       except in the beginning.

 10. Limitations on Two-dimensional Code
     - With some applications, the space character in two-byte within the
       character string specified may be printed in one-byte.




7. Others

  1. The emulation for this driver is in the "ESC/P2" mode.
     Make sure the setting of the printer installation corresponds to it.

  2. Users are required to adjust devices for such as the paper insertion.
     Please make sure the paper settings, as well as the settings from the
     operation panel correspond to the printer.

  3. Printing from other Windows application software under the other Windows
     environments may give different results.

  4. The contents of "Properties" of the printer driver and "Printing
     Preferences" of the printer may overlap.
     Please make necessary adjustments to avoid any possible malfunction.

  5. user-defined papers
     - Paper size from the "Server Properties" can be set to a maximum width
       of 15 inches. Adjust the right and left margins not the exceed an 13.6
       inch paper width as the data may not be properly printed.
     - The paper length can be set starting from 1inch (about 25.4 mm).
       However, when specifying any of the paper feed ports below, do not
       specify paper 2.76 inches (about 70.0 mm) or less in length.
       Otherwise, the paper will not be properly fed, leading to a paper jam.
       - manual feed
       - CSF #1
       - CSF #2

  6. When printing with a "Page per Sheet" specification from the "layout" tab
     in the print menu, frame lines may not be printed with some applications.

  7. If printing is cancelled from the printer port during printing, restart
     the printer.
     Continuing printing without restarting the printer may result in problems
     such as garbled texts.

  8. Continuous forms
     - Both the upper and lower margins for continuous form are set at 0mm in
       this printer driver.  It is recommended that the upper and lower margins
       for continuous form using Tractor feeder with this printer is more than
       25.4mm.
     - The printing head and the ribbon may be damaged when printing on the
       perforation lines and sprocket holes.
     - Paper with a length of 3 inches-14 inches isruled with a width of 15
       inches. When using paper with a width less than 15 inches, please make
       adjustments to the right margin of the application not to exceed the
       maximum possible range.
     - When using Continuous form with a tractor feeder on this printer, the
       possible folding length is 4 inches or more.
       When the folding length is the same as the page length, use paper with
       a folding length of more than 4 inches.

  9. Envelopes
     - Print only on the surface side.  Do not print on the flap side as the
       envelope may be jammed.
     - Do not print on envelopes with a window or double-layered envelopes.
     - Both the top and bottom margins are set at 25.4mm in this printer
       driver.
     - Printing outside the margin out of guarantee.
     - Refer to the following for paper-feeding directions to avoid a paper
       jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

 10. Cut sheets
     - Adjust the paper guide when printing on A3 Rotated paper.
       (The left printing margin is set at 38mm)

 11. The DL7600Pro/DL7400Pro printer driver to every connecting port will
     be set if the connecting USB port is changed.  (e.g. FUJITSU DL7600Pro
     (copy 2) etc.)
     Since every setting of the printer driver is the initial value, so
     change the setting according to the using state.
     ** In this section, FUJITSU DL7600Pro printer driver is used as an
        example.

 12. Changing the paper feed port or paper size with the page setting or
     document setting in the application.
     The margin size outside the print enabled area can be set even when the
     printer driver specified value is not correctly reflected.
     To prevent this, first set the paper feed port and paper size you intend
     to use with printer properties in the printer folder.
     Then change the paper feed port and paper size in the application, or
     avoid setting the margin size outside the print enabled area.
     For information on the print enabled area (minimal margin size) per
     individual paper feed ports and paper sizes, refer to the Users Manual.

 13. Regarding the DL7600Pro/DL7400Pro Printer
     Ejecting cut sheet paper to the cut sheet table in front sometimes leads
     to wait for removal of a cut sheet (blinking lamp for ejection in front).
     In such cases, remove the paper from the cut sheet table, load the next
     paper, and then press the online switch.
     ** The error message displayed when status of wait for removal of a cut
        sheet (blinking lamp for ejection in front) occurs during printing 
        indicates a time out error, not a paper out error.

 14. When Printer Font is specified and print it, change language setting to
     "WCP1252" and character setting to "GRAPHIC" by DLMENU or Offline Setup.
     Otherwise, print result may not be correct.



- About the trademark
  Company names and product names mentioned above are registered trademarks
  or trademarks of each company.

[End]
