
 << Sorry for English >>

==============================================================================
                             Microsoft Windows 7

                         FUJITSU DL7600 Printer Driver

                    Copyright(C) 2010 FUJITSU ISOTEC LIMITED
==============================================================================

This printer driver works on the following operating systems:

  Windows(R) 7 Ultimate,
  Windows(R) 7 Ultimate x64 Edition,
  Windows(R) 7 Enterprise,
  Windows(R) 7 Enterprise x64 Edition,
  Windows(R) 7 Professional,
  Windows(R) 7 Professional x64 Edition,
  Windows(R) 7 Home Premium,
  Windows(R) 7 Home Premium x64 Edition,
  Windows(R) 7 Starter
  -> referred to as Windows 7

This printer driver is for FUJITSU DL7600 printers.



Content

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup method using Add Printer Wizard
  3.3 Using Plug & Play
4. Uninstalling the printer driver
5. Printer driver setup method
6. Others
- About the trademark

Note: This driver is for FUJITSU DL7600 printers.
      Do not use with other printers.
      When printing using Windows 7, change the printer settings back to
      the factory default.
      Otherwise the printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the Windows 7

- Operating system
  Windows 7



2. Printer driver configuration

  FUJITSU DL7600 printer driver consists of the following files:

   DL7600.DLL     FUJITSU DL7600 printer driver resource DLL file
   DL7600.GPD     FUJITSU DL7600 printer driver GPD file
   HGLMONN.DLL    FUJITSU DL7600 Language Monitor
   DL7600.INF     Setup information file
   README.TXT     This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) Windows 7
   2) Printer Driver Disk (this disk)

- When setting up, log on with an Administrator account.

- After inserting the Setup Disk into your PC’s CD-ROM drive, the FUJITSU DL
  Series Software setup window is displayed.
  If your operating system is Windows 7, click the OK button.
  For any other Windows operating system, click the Exit button.

- If the FUJITSU DL7600 printer driver has already been set up,
  delete it and set up again.

- This guide includes procedures on installing printer drivers on locally
  connected PC's.
  For installation methods on network connection and shared printers, refer to
  the Windows 7 user's manual or "help".

- During setup, in the User Account Control dialog box, you may be asked, Do
  you want to allow the following program from an unknown publisher to make
  changes to this computer ? Select Yes.

- When using 64-bit Windows 7, follow the above procedure also.


-----------------------------------------
3.2 Setup method using Add Printer Wizard
-----------------------------------------
Use the Add Printer Wizard to set up the printer driver.
In this section, the setup procedure for Windows 7 is described.
In the following procedure, Fujitsu DL7600 printer driver is set up.
When using another printer or another printer driver, change it to your current
printer or printer driver name to follow the procedure.

 1. Log on as an administrator of the computer.

 2. Select Start, and then select Devices and Printers. 

 3. From the Devices and Printers folder, select Add a printer. 

 4. The Add Printer Wizard is displayed. Select Add a local printer. 

 5. Specify a port to connect the printer to and click the Next button.
    ** If a port is not available, for example, in a case where a port to
       connect the printer is not present in the list of Use an existing port,
       select a temporary port such as LPT1:(Printer Port) instead.

 6. The window of Install the printer driver is displayed. Click Have Disk.

 7. Insert the Setup CD-ROM into CD drive (D:). Then, change the path name from
    "A:\" to "D:\DL7600\Win7" and click the OK button.
    ** The CD drive is set to "D:" in the above example.
       If your CD drive is set to another driver, change the path to the
       correct drive.
    ** For 64-bit Windows 7, the above folder should be specified as well.
    ** When installing another printer driver, change the printer driver part
       to your model’s printer drive name in the path to specify.
    ** When using the latest printer driver downloaded from our web site, type
       "(a folder name where downloaded driver data is present)\Win7".

 8. The model names are displayed in the list box.
    Select the printer driver to use and click Next. 
    ** When the window containing the message, Which version of the driver do
       you want to use ?, is displayed, select Replace the current driver.

 9. The dialog Type a printer name is displayed. Type the printer name and
    click Next.
    ** To change the printer name, key-in the changed printer name.

10. In the Windows Security dialog box, the message, Windows can’t verify the
    publisher of this driver software is displayed. Select Install this driver
    software anyway.

11. A file copy starts.

12. The Printer Sharing Window is displayed. Select according to your computer
    environment and click the Next button.
    ** The Printer Sharing Window may not be available for some computer
       environments.
    ** When the Printer Sharing Window is displayed, select according to your
       computer environment.
       (1) Not sharing : Select Do not share this printer. 
       (2) Sharing     : Select Share this printer so that others on your
                         network can find and use it and enter Share name,
                         Location, and Comment.

13. Make sure that the message, You've successfully added Fujitsu DL7600, is
    displayed, and click the Finish button to terminate the wizard.
    ** If multiple printer drivers have been installed, this window will
       display the item, Set as the default printer. Select as needed.
    ** In this window, Print a test page is displayed. If required print a
       test page.
    ** Notes on test page printing
       (1) When a temporary port is selected in Procedure 5., do not print any
           test page.
       (2) Make sure that the printer is online when printing test pages.
       (3) Test pages are printed according to the printer driver settings at
           that point.
           In the printer driver default, Paper Source: Automatically Select
           and Paper Size: 11 inch Stockform(W:15in) are configured.
           Print test pages with 11 inch Stockform.
       (4) To use a non-default feed method or paper size, change the setting
           first, and then print test pages.

14. Restart Windows. This completes the printer driver setup.

When the printer is connected after the setup in this method, the dialog
Installing device driver software may be displayed and the connected printer
may be displayed under Unspecified part of Devices and Printers.
In that case, restart Windows. 


---------------------
3.3 Using Plug & Play
---------------------

[IMPORTANT Before setting up]
  For Windows 7 , install the printer driver before connecting the printer to
  your personal computer.
  Either of the following messages is displayed in the setup program: Printer
  is ready for installation. or Printer driver installation has been completed.
  After the message is displayed, connect the printer to your PC.

Require: 
  Be sure to turn off the power to both the computer and the printer.

 1. Log on as an administrator of the computer.

 2. Insert the Setup Disk into your PC’s CD-ROM drive. The Auto Play window
    will be displayed. Click Run DLSELECT.EXE.
    If the Auto Play window is not displayed, use Explorer or another
    application to open CD-ROM.  and double click the DLSELECT.EXE file.

 3. The FUJITSU DL Series Software Setup window is displayed. From the printer
    driver list, select DL7600 and click the OK button.
    ** When using the latest printer driver downloaded from our web site,
       double click the executable program (a file whose extension is EXE)
       in the downloaded driver data folder.

 4. When the dialog box, Do you want to allow the following program from an
    unknown publisher to make changes to this computer ? is displayed, click
    Yes.

 5. The FUJITSU DL Series Printer Driver Package window is displayed.
    Click the OK button.

 6. Select a printer driver to add will be displayed.
    To use a network port, check mark the option "Use a network port."

 7. Follow the display menu and select a printer driver to install.
    Then, click the OK button. 
    ** If selecting Use a network port, go to step a.
    ** If you do not wish to install the printer driver, select Cancel.
       When the procedure is ended without any printer driver installation,
       double click each executable program of FUJITSU DL Series Software Setup
       or FUJITSU DL Series Printer Driver Package again or install the printer
       driver through Setup method using Add a Printer Wizard.
    ** About "Use a network port"
       (1) For creation or setup method of a network port, read the manual or
           setup guide of an optional LAN board or LAN adapter or see the Help
           topic in Windows 7 .
       (2) When using a network port created through an optional LAN board or
           LAN adapter or using Windows Standard TCP/IP port, select this item.
       (3) Do not select this item when using a parallel port or a USB port.

 8. In Windows Security dialog box the dialog, Windows can’t verify the
    publisher of this driver software is displayed.
    Select Install this driver software anyway.

 9. A file copy starts.
    ** Wait until the message Printer driver is ready for installation.

10. Once the message, Printer driver is ready for installation, is displayed
    Click the OK button.

11. Connect the printer to your PC and turn on the printer power.

12. Installing device driver software is displayed in the taskbar notification
    area.
    After a while, the message Fujitsu DL7600 Device driver software installed
    successfully is displayed.
    ** When a USB interface is used for connection the message Your device is
       ready to use is displayed instead.

13. Select Start, and then select Devices and Printers.

14. Make sure that the printer driver icon is added to Printers and Faxes
    section.

15. Restart Windows.

[When Use a network port is selected:]
a. The following message is displayed: Use a network port is selected.
   Read the instructions carefully and click the OK button.

b. In the Windows Security dialog box, the message, Windows can't verify the
   publisher of this driver software is displayed, select Install this driver
   software anyway.

c. A file copy starts. 
   ** Wait until the window of Procedure D. is displayed.

d. The Add Printer Wizard is displayed. Select Add a local printer.

e. Specify a port to connect the printer and click Next.
   ** If a port is not available, for example, in cases where a network port
      to use is not present in the list of Use an existing port, select a
      temporary port such as LPT1:(Printer Port).

f. The dialog Install the printer driver is displayed. From Manufacturer,
   select FUJITSU. From the list of Printers, choose a model to use and click
   the Next button.

g. The dialog Type a printer name is displayed. Type the printer name and click
   the Next button.
   ** When changing the printer name, key-in the changed printer name.

h. A file copy starts. 
   ** Wait until the window of Procedure I. or Procedure J. is displayed.

i. The Printer Sharing Window is displayed. Select according to your computer
   environment and click the Next button.
   ** The Printer Sharing Window may not be displayed for some computer
      environments.
      When the Printer Sharing Window is displayed, select according to your
      computer environment.
      (1) Not sharing : Select Do not share this printer. 
      (2) Sharing     : Select Share this printer so that others on your
                        network can find and use it and enter Share name,
                        Location, and Comment.

j. Make sure that the message, You've successfully added Fujitsu DL7600, is
   displayed, and click the Finish button to terminate the wizard.
   ** When multiple printer drivers have been installed, Set as the default
      printer is displayed. Select as needed.
   ** In this window, the Print a test page button is displayed. If required
      print a test page.
   ** Notes on test page printing
      (1) When a temporary port is selected in Procedure E., do not print any
          test page.
      (2) Make sure that the printer is online when printing test pages.
      (3) Test pages are printed according to the printer driver settings at
          that point.
          In the printer driver default, Paper Source: Automatically Select
          and Paper Size: 11 inch Stockform(W:15in) are configured.
          Print test pages with 11 inch Stockform.
      (4) To use a non-default feed method or paper size, change the setting
          first and then print test pages.

k. The following message is displayed: Printer driver installation has been
   completed.
   Read the instructions carefully and click the OK button.

l. Select Start, and then select Devices and Printers.

m. Make sure that the printer driver icon is added to Printers and Faxes
   section.

n. Restart Windows. This completes the printer driver setup.



4. Uninstalling the printer driver

   The following procedure is used to delete the printer driver. 

   -NOTE-
   ** In this section, FUJITSU DL7600 printer driver is used as an example.
   ** When using another printer driver, change the name to your current
      printer driver name to read the description.
   ** To delete, make sure the printer driver is not in use. If any printing
      is in progress, cancel the printing job.

 1. Select Start, and then select Devices and Printers.

 2. Select Fujitsu DL7600 under Printers and Faxes. Then, select Remove device.

 3. The dialog Remove device is displayed. The message, Are you sure you want
    to remove this device? Fujitsu DL7600, is displayed. Select Yes.

 4. Select the installed printer under Printers and Faxes such as Fax or
    Microsoft XPS Document Writer. Then, select Print server properties.

 5. Click the Drivers tab and click the Change Driver Settings button.
    ** For some log-on accounts, such as a built-in administrator account, this
       button may not be displayed.

 6. From the Installed printer drivers list, select Fujitsu DL7600 and click
    the Remove button.

 7. The Remove Driver and Package dialog is displayed. Select Remove driver and
    driver package and click the OK button.

 8. The window containing the message, Deleting this printer driver package
    will remove it from the system. Are you sure you want to delete Fujitsu
    DL7600 ?, is displayed. Click Yes.

 9. In the Remove Driver and Package dialog, the following message is
    displayed: Driver package information collected. Click the Delete button.

10. When the message, Driver package deleted. is displayed, click the OK
    button. 
    Then, click the Close button to terminate the Print server properties
    dialog box.

11. Turn off the printer’s power and restart Windows 7.

This completes the printer driver removal.
When the following message is displayed in Procedure 10.: This package
contains the following driver(s) that are in use:, restart Windows 7 and
remove the printer driver again.



5. Printer driver setup method

- Document properties such as paper size and others can be set in the "printer
  properties" menu in the application software.

- Depending on the application software used, the paper size settings
  of the application software may be the default rather than that of the
  "page setting" tab.

- How to assign paper size etc to each paper feed is as follows.
  In this section, FUJITSU DL7600 printer driver is used as an example.
  When using another printer driver, change it to your current printer driver
  name to follow the procedure.
  (1) Select Start, and then select Devices and Printers.
  (2) Right click on Fujitsu DL7600 displayed under Printers and Faxes and
      select Printer properties.
      Then, specify in the Form To Tray Assignment section under the Device
      Settings tab.
      NOTE:
      - This method is valid only when the Paper Source setting of the printer
        driver is set at the "Automatically Select".
      - Please make sure the actual paper size matches the selected paper size.
        Use the "Manual Paper Feed" the actual paper size differs from the
        selected paper size.

- How to create a user-defined paper size is as follows.
  In this section, Fujitsu DL7600 printer driver is used as an example.
  When using another printer driver, change it to your current printer driver
  name to follow the procedure.
  (1) Log in with an administrator group account.
  (2) Select Start, and then select Devices and Printers.
  (3) Click Fujitsu DL7600 displayed under Printers and Faxes and select Print
      server properties on the menu bar.
  (4) Click the Change Form Settings button under the Form tab.
  (5) Check mark Create a new form.
  (6) Type a paper name to create in Form name.
  (7) Select a unit of the paper size to create under Form description
      (measurements) and enter the width and the height of the paper.
  (8) Click Save Form.
  (9) Click the OK button and close Print server properties.
  NOTE:
  - For some versions of Windows 7, the procedure or display contents may vary.
    In that case, follow the displayed instructions.
  - Use inch as a unit to specify the length if you can.
  - If a special continuous paper form such as paper length with 10, 11, 13,
    14, 16, or 17 inches in 3 pages as a user-defined size is created or
    configured, an error may occur. This may result in a printing misalignment.
  - For a user-defined size, even after its margins are correctly set, it may
    not be reflected properly. Edit margins in Page Setting in the application.



6. Others

a. The emulation for this driver is in the "ESC/P2" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from other Windows application software under the Windows 7
   environments may give different results.

d. The contents of "Properties" of the printer driver and "Printing
   Preferences" of the printer may overlap.  Please make necessary adjustments
   to avoid any possible malfunction.

e. Some specified printer fonts from the application may not be used depending
   on the data format.

f. Paper size from the "Server Properties" can be set to a maximum width of
   15 inches.  Adjust the right and left margins not the exceed an 13.6 inch
   paper width as the data may not be properly printed.

   The paper length can be set starting from 1inch (about 25.4 mm).
   However, when specifying any of the paper feed ports below, do not specify
   paper 2.76 inches (about 70.0 mm) or less in length.
   Otherwise, the paper will not be properly fed, leading to a paper jam.
   - manual feed
   - CSF #1
   - CSF #2

g. When printing with a "Page per Sheet" specification from the "layout" tab in
   the print menu, frame lines may not be printed with some applications.

h. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

i. Paper with a length of 3 inches - 14 inches isruled with a width of 15
   inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

j. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

k. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

l. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

m. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

n. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

o. The DL7600 printer driver to every connecting port will be set if the
   connecting USB port is changed.  (e.g. FUJITSU dl7600 (copy 2) etc.)
   Since every setting of the printer driver is the initial value, so
   change the setting according to the using state.

p. When Printer Font is specified and print it, change Language setting
   to WCP1252 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.

q. Regarding the DL7600 Printer
   Ejecting cut sheet paper to the cut sheet table in front sometimes leads to
   wait for removal of a cut sheet (blinking lamp for ejection in front).
   In such cases, remove the paper from the cut sheet table, load the next
   paper, and then press the online switch.

   ** The error message displayed when status of wait for removal of a cut
      sheet (blinking lamp for ejection in front) occurs during printing 
      indicates a time out error, not a paper out error.

r. Changing the paper feed port or paper size with the page setting or
   document setting in the application.
   The margin size outside the print enabled area can be set even when the
   printer driver specified value is not correctly reflected.
   To prevent this, first set the paper feed port and paper size you intend to
   use with printer properties in the printer folder.  Then change the paper
   feed port and paper size in the application, or avoid setting the margin
   size outside the print enabled area.  For information on the print enabled
   area (minimal margin size) per individual paper feed ports and paper sizes,
   refer to the Users Manual.



- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
